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	Start Work Authority: Confirm below are in place and verified prior to starting work
	

	Save Your Life Actions
All exposed person(s) performing work must confirm each of the action items below
	Person(s) Performing Work (initial)
	Start-Work 
Verifier 
(initial)
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	I have confirmed:
	

	1
	Circuit, system, and/or equipment to be de-isolated/re-energized is the one identified in the isolation plan or drawing.
	
	
	

	2
	Isolation devices are removed per the isolation plan or drawing.
	
	
	

	3
	Any personnel affected by the re-energizing activity have been notified.
	
	
	

	4
	The circuit, system, and/or equipment has been re-energized per plan or drawing.
	
	
	

	Stop and seek help if any of the above controls/safeguards are not in place
	

	
	

	Role
	Printed Name
	Date
	

	Start -Work Verifier
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	Start Work Authority: I will not start work until I confirm…

	Actions
	How to (examples)

	1
	Circuit, system, and/or equipment to be de-isolated/re-energized is the one identified in the isolation plan or drawing.
	• Tags or markings identify the circuit, system and/or equipment to be de-isolated/re-energized.

Note: Confirm circuit, system, and/or equipment is ready to be de-isolated and re-energized (e.g. all work has been completed)

	2
	Isolation devices are removed per the isolation plan or drawing.
	• Physically inspect:  
     • Work area to confirm all mechanical, process and electrical isolations were removed per plan.
     • Bleed and vent points to confirm they are closed/open per plan or procedure.

	3
	Any personnel affected by the re-energizing activity have been notified.
	• Personnel in/near the work area or affected by the re-energizing of circuit, system, and/or equipment are aware it is ready to be put back in service. 
• Personnel are not in the Line of Fire of re-energized potential hazardous energy sources (e.g., electrical, pressure, hydraulic, mechanical etc)

	4
	The circuit, system, and/or equipment has been re-energized per plan or drawing.
	• Circuit, system, and/or equipment has been re-energized per the isolation plan or system/equipment operating procedure.
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