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	Start Work Authority: Confirm below are in place and verified prior to starting work
	

	Save Your Life Actions
All exposed person(s) performing work must confirm each action below
	Person(s) Performing Work (initial)
	Start-Work 
Verifier 
(initial)
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	I have confirmed:
	

	1
	Equipment to be demolished is emptied/cleared of hazardous materials.
	
	
	

	2
	All energy sources are identified, isolated and marked / colour coded.
	
	
	

	3
	Equipment that may have stored energy is identified and marked.
	
	
	

	4
	Safe areas, out of the line of fire are identified, with barriers in place where practical.
	
	
	

	5
	Work area is assessed for potential dropped or unsecure objects, and potential objects have been removed or secured.
	
	
	

	6
	Residual contaminants have been identified, and appropriate PPE and work methods provided.
	
	
	

	Stop and seek help if any of the above safeguards are not in place
	

	
	

	Role
	Printed Name
	Date
	

	Start -Work Verifier
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	Start Work Authority: I will not start work until I confirm…

	Actions
	How to (examples)

	1
	Equipment to be demolished is emptied/cleared of hazardous materials.
	(e.g. hydrocarbons, chemicals, contaminants, NORM, etc.).

	2
	All energy sources are identified, isolated and marked / colour coded.
	(e.g. electrical, pressure, gravity, etc.)

	3
	(e.g. spring-loaded equipment, bent or obstructed materials, valves, pipe, suspensions, loading arms)
	(e.g. spring-loaded equipment, bent or obstructed materials, valves, pipe, suspensions, loading arms)

	4
	Safe areas, out of the line of fire are identified, with barriers in place where practical.
	unforeseen equipment, materials movement

	5
	Work area is assessed for potential dropped or unsecure objects, and potential objects have been removed or secured.
	objects that may become loose / unsecure during the demolition process and have the potential to cause harm.

	6
	Residual contaminants have been identified, and appropriate PPE and work methods provided.
	(e.g. Lead, Asbestos, PCB's, etc.)
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