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	Start Work Authority: Confirm below are in place and verified prior to starting work
	

	Save Your Life Actions
All exposed person (s) performing work must confirm each of the action items below
	Person(s) Performing Work (initial)
	Start-Work 
Verifier 
(initial)
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	I have confirmed:
	

	1
	The circuit, system, and/or equipment to be worked on, is identified in the isolation plan or drawing.
	
	
	

	2
	All hazardous energy sources have been identified.
	
	
	

	3
	Isolation points are identified per the isolation plan and/or drawing. 
	
	
	

	4
	Isolation devices are set in the identified position per isolation plan or drawing.
	
	
	

	5
	The locks and tags are installed on the equipment/devices per the isolation plan.
	
	
	

	6
	Zero energy state has been verified, proven and demonstrated.
	
	
	

	Stop and seek help if any of the above controls/safeguards are not in place
	

	
	

	Role
	Printed Name
	Date
	

	Start -Work Verifier
	
	
	




	[image: ]   Save Your Life Actions |  Energy Isolation 

	Start Work Authority: I will not start work until I confirm…

	Actions
	How to (examples)

	1
	The circuit, system, and/or equipment to be worked on, is identified in the isolation plan or drawing.
	• Tags or markings identify the circuit, system and/or equipment indicated by the isolation plan or drawing. 

	2
	All hazardous energy sources have been identified.
	• Complete a task risk assessment specific to the scope of work
• Discuss hazards with the work team prior to starting work
• Inspect equipment for potential energy sources (e.g., electrical, pressure, hydraulic, mechanical, etc.)
• Identify and mitigate hazards on any nearby energized circuit/systems/equipment

	3
	Isolation points are identified per the isolation plan and/or drawing. 
	• All isolations points are in place and tagged or marked (i.e., use isolation diagram, Equipment Isolation Procedure, P&IDs, or Process Flow Diagrams). 

	4
	Isolation devices are set in the identified position per isolation plan or drawing.
	• Valves are open or closed per the diagram and/or plan.
• Blinds, spades and skillets are:
      • stamped or certified for the pressure rating of the equipment.  
      • installed per the diagram and/or plan
• Electrical isolation points are open/switched off or disconnected from power source

	5
	The locks and tags are installed on the equipment/devices per the isolation plan.
	• All isolations are in place and tagged or marked (i.e., use isolation diagram, Equipment Isolation Procedure, P&IDs, or Process Flow Diagrams). 
• Lock out tagout devices are on isolation points 
• Keys are in a designated secure location

Note: If a lock is unable to be placed, confirm hazardous energy source(s) points are isolated and secured per isolation plan.

	6
	Zero energy state has been verified, proven and demonstrated.
	• Demonstrate powered equipment cannot be started. 
• Systems (lines, gauges, etc.) have been tested for residual or stored energy by: 
      • Check bleed and vent points are open to release stored energy 
      • Check gauges, measurements & volt meters 

Note: If zero energy is not possible, STOP and
      • Confirm controls/safeguards are in place, functioning, operated and maintained to manage the risk from residual energy



Page 1

image1.png




image2.jpeg




