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	Start Work Authority: Confirm below are in place and verified prior to starting work
	

	Save Your Life Actions
All exposed person(s) performing work must confirm each of the action items below
	Person(s) Performing Work (initial)
	Start-Work 
Verifier 
(initial)
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	 Energy Isolation
	

	I have confirmed:
	

	1
	The confined space has been evaluated for energy isolation requirements.
[image: ][image: ]Does Confined Space Entry work require energy isolation? 
Yes:       No:
If yes: Complete Energy Isolation Start-Work Check.
If no: Continue to Step 2.
	
	
	

	Prior to Confined Space Entry
	

	I have confirmed:
	

	2
	The hazards have been identified, controlled and it is safe to start.
	
	
	

	3
	Gas testing frequency has been established.
	
	
	

	4
	Ventilation is in place and working.
	
	
	

	5
	An attendant is in place and the method of communication is agreed to and tested prior to entry.
	
	
	

	6
	My breathing apparatus is in good working condition.
If no breathing apparatus is required: Continue to the next step.
	
	
	

	7
	The rescue plan is in place and ready to be used.
	
	
	

	Stop and seek help if any of the above controls/safeguards are not in place
	

	
	

	Role
	Printed Name
	Date
	

	Start -Work Verifier
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	Start Work Authority: I will not start work until I confirm…

	Actions
	How to (examples)

	Energy Isolation

	1
	The confined space has been evaluated for energy isolation requirements.
Does Confined Space Entry work require energy isolation? 
Yes:       No:
If yes: Complete Energy Isolation Start-Work Check.
If no: Continue to Step 2.
	• All potential energy sources have been identified, isolated and locked and tagged per isolation plan. 
• The system has been drained, flushed, or purged to remove explosive materials or gases.

	Prior to Confined Space Entry

	2
	The hazards have been identified, controlled and it is safe to start.
	• Complete a task risk assessment specific to the scope of work
• Discuss hazards with the work team prior to the start of work
• Check for simultaneous operations that may introduce an additional hazards

	3
	Gas testing frequency has been established.
	• Gas testing is being done by a Qualified Gas Tester
• Initial gas testing and the required follow up testing frequency before starting work. 
• Check testing results and agree on a schedule for follow-up testing before starting work

	4
	Ventilation is in place and working.
	• Confined space is continuously ventilated
• If using mechanical ventilation: 
      • The flexible ducting is arranged so there is continuous air flow in the entire space.  
      • Equipment is bonded and grounded to prevent static electricity hazards. 
• Ventilation inlets: 
      • are not near an ignition source.
      • will not be affected by wind/weather conditions and will not have flow restrictions.
      • will not draw contaminated air into the space (e.g., vehicle, generator exhaust). 

	5
	An attendant is in place and the method of communication is agreed to and tested prior to entry. 
	• Dedicated attendant is present at the designated entry point(s) to the confined space. 
• Ask the attendant to describe their responsibilities, which include: 
      • Using previously agreed upon communication methods (e.g., hand signals, radio)     
      • Monitoring personnel in the confined space 
      • Documenting entry and exits from the confined space  
      • Monitoring the confined space for changing conditions
      • Initiating the emergency rescue response if needed  

	6
	My breathing apparatus is in good working condition.

If no breathing apparatus is required: Continue to the next step.
	• The breathing apparatus is complete, certified, in good working condition 
• The main air supply is correct and properly connected before using it.
• Escape pack is in place and functioning prior to entry.

	7
	The rescue plan is in place and ready to be used.
	•Discuss method of communication with attendant & rescue team prior to entry.
•Rescue equipment is at the job site 
•The entrant is wearing rescue equipment per plan (e.g., harnesses, retrieval device).
• The rescue crew: 
       • is available
       • is aware of specific hazards related to this task
       • can execute the rescue plan
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